

BAR CODE MEDICATION ADMINISTRATION (BCMA)

INSTALLATION GUIDE

Version 3.0

February 2004

(Revised May 2021)

Department of Veterans Affairs

**V***IST***A** Health Systems Design & Development

Revision History

| Date | Patch | Description |
| --- | --- | --- |
| 05/2021 | PSB\*3\*123 | [BCMA and BCMA Parameters are being converted to Delphi XE10.4 to make them TRM Compliant, and several reported defects were resolved.](#PSB_3_96_ClientFilesDistDuringBCMA_V3In)Liberty ITS |
| 12/2019 | PSB\*3\*101 | [PSB\*3\*101 addresses reported defects in BCMA and BCMA parameters applications.](#PSB_3_96_ClientFilesDistDuringBCMA_V3In) REDACTED |
| 5/2019 | PSB\*3\*118 | [BCMA is being converted to Delphi XE10 and made Windows 10 compatible](#PSB_3_96_ClientFilesDistDuringBCMA_V3In)REDACTED |
| 12/2018 | PSB\*3\*96 | [Two-factor authentication (2FA) patch for BCMA is releasing a dll, OrderCom.dll, that is replacing the BCMAOrderCom.dll.](#PSB_3_96_ClientFilesDistDuringBCMA_V3In)REDACTED |

Table of Contents

[BCMA V. 3.0 and This Guide 1](#_Toc65900710)

[Benefits of BCMA V. 3.0 1](#_Toc65900711)

[Patient Transfer Notification Message 4](#_Toc65900718)

[Documenting Fractional Dose Orders 4](#_Toc65900719)

[BCMA Clinical Reminders Marquee 4](#_Toc65900720)

[PRN Documentation Site Parameter 5](#_Toc65900723)

[Include Schedule Types Site Parameter 5](#_Toc65900724)

[Accessing PRN Effectiveness Log 5](#_Toc65900725)

[Schedule Type Indicator Alert Lights 6](#_Toc65900728)

[Medication Log Dialog Box 6](#_Toc65900729)

[PRN Effectiveness Dialog Box 6](#_Toc65900730)

[Scan IV Dialog Box 6](#_Toc65900731)

[Bag Information Column on VDL 6](#_Toc65900732)

[Report Printing 7](#_Toc65900735)

[HL7 Messaging 8](#_Toc65900738)

[Missing Dose E-Mail Notification 8](#_Toc65900739)

[Documenting PRN Pain Scores 8](#_Toc65900740)

[Administering a Multiple Dose Order 9](#_Toc65900743)

[Administering a PRN Order 9](#_Toc65900744)

[Recording the Effectiveness of a PRN Medication 9](#_Toc65900745)

[Creating Default Answers Lists 9](#_Toc65900746)

[Benefits of This Guide 10](#_Toc65900748)

[Our Target Audience 10](#_Toc65900749)

[Other Sources of Information 10](#_Toc65900750)

[Background/Technical Information 10](#_Toc65900751)

[This Manual and Related Documentation 10](#_Toc65900752)

[Documentation Retrieval Process 11](#_Toc65900754)

[Conventions Used in This Guide 12](#_Toc65900756)

[Obtaining On-line Help 14](#_Toc65900760)

[Locating Detailed Listings 14](#_Toc65900761)

[Routines 14](#_Toc65900762)

[Data Dictionaries 14](#_Toc65900763)

[Pre-Installation Information 15](#_Toc65900764)

[Minimum Required Packages 15](#_Toc65900765)

[Installation Time Estimates 15](#_Toc65900766)

[Resource Requirements 16](#_Toc65900768)

[Response Time Monitor 16](#_Toc65900769)

[Laptops and Bar Code Scanners 16](#_Toc65900770)

[Printers 16](#_Toc65900771)

[Unit Dose Label Printer Devices 16](#_Toc65900772)

[IV Label Printer Devices 16](#_Toc65900773)

Table of Contents

[Pre-Installation Information (cont.)](#_Toc65900764)

[Client PC Setup Requirements 17](#_Toc65900775)

[Files Required to Run BCMA V. 3.0 17](#_Toc65900776)

[Routines Installed 18](#_Toc65900778)

[Routine Mapping 18](#_Toc65900779)

[Routines with Related Checksums 19](#_Toc65900781)

[Installation Information 21](#_Toc65900783)

[V*IST*A Server Installation Instructions 21](#_Toc65900784)

[Task 1: Download BCMA V. 3.0 Software 21](#_Toc65900785)

[Task 2: Load the KIDS Distribution File 22](#_Toc65900788)

[Task 3: Install BCMA V. 3.0 22](#_Toc65900789)

[Additional Preparation for BCMA V. 3.0 23](#_Toc65900793)

[Working with GUI BCMA V. 3.0 25](#_Toc65900794)

[Client PC Setup Requirements 25](#_Toc65900795)

[Client Distribution Files 25](#_Toc65900796)

[Standard Installation Procedure for GUI BCMA V. 3.0 26](#_Toc65900798)

[Working with the Hosts File on the Client PC 27](#_Toc65900800)

[Setting up Optional Command Line Parameters 28](#_Toc65900802)

[Working with the Monthly SAGG Report 29](#_Toc65900803)

[Setting up the Monthly Batch Job 29](#_Toc65900804)

[Glossary 33](#_Toc65900809)

[Learning BCMA V. 3.0 Lingo 33](#_Toc65900810)

[APPENDIX A: Sample KIDS Load & Installation 35](#_Toc65900813)

# BCMA V. 3.0 and This Guide

|  |  |
| --- | --- |
| Benefits of BCMA V. 3.0tip:**The BCMA Virtual Due List (VDL)** is called “BCMA VDL” in this guide to eliminate confusion withthe V*IST*A Documentation Library (VDL)also mentionedin this guide.j0255778 | This section lists the National Online Information System (NOIS)tickets that are corrected in Bar Code Medication Administration (BCMA) V. 3.0, and provided in the Build description.1. **Problem:** NOIS ISB-0603-31561A medication order that has administration times set for today, but before the Start Time of the order, displays on the Bar Code Medication Administration (BCMA) Due List Report.**Corrective Action:**The Due List Report will not display medication orders until the Start Date/Time of the medication order takes effect.
2. **Problem:** NOIS ISB-0903-31964When the user selects a time frame for the Medication Administration History (MAH) Report and no administrations are due, the report lists the medication order number from Inpatient Medications V. 5.0 under the “Initial – Name Legend” section.**Corrective Action:** The MAH Report will not display the order number from Inpatient Medications V. 5.0 under the “Initial – Name Legend” section when no administrations are due for a specific time frame.
3. **Problem:** NOIS LAH-1203-61493The user receives the following error message, “BCMA failed to communicate with VISTA,” if the Graphical User Interface (GUI) BCMA times out and is unable to connect to the server.**Corrective Action:** The processing time for the GUI BCMA software to display the patient’s record on the BCMA Virtual Due List (VDL) has been reduced.
4. **Problem:** NOIS LIT-0603-71923Users sometimes receive an “allocation failure” error message when accessing a patient’s record using the GUI BCMA.**Corrective Action:** The “allocation failure” error message has been corrected.
 |

BCMA V. 3.0 and This Guide

|  |  |
| --- | --- |
| Benefits ofBCMA V. 3.0 (cont.) | 1. **Problem:** NOIS MAD-1203-42204The MAH Report takes an extended amount of time to run if the Start Date and the Stop Date of the report, requested by the user, are for different years. For example, if the Start Date is 12/28/03 and the Stop Date is 01/03/04.**Corrective Action:** The user can now request different years for the MAH Report without experiencing extended delays as BCMA accesses the data.
2. **Problem:** NOIS MIN-1203-41637Users sometimes experience an “Invalid Medication Lookup” error message after scanning a medication in the “Scan Medication Bar Code:” field of the “Order Manager” dialog box when using the BCMA Med Order Button in GUI BCMA.**Corrective Action:** The BCMA medication lookup process has been corrected to properly validate the medications scanned in the “Scan Medication Bar Code:” field of the “Order Manager” dialog box in GUI BCMA.
3. **Problem:** NOIS UNY-0104-10174Multiple IV medication orders display as merged on the IV Medication Tab after an order is discontinued, but the IV bag is still infusing.**Corrective Action:** Multiple IV medication orders will display properly on the IV Medication Tab.
4. **Problem:** NOIS TNV-0104-30647Users sometimes experience the following error message, “ERROR: 16^Server Protocol Disabled,” when using the Edit Medication Log [PSB MED LOG EDIT] option. This occurs when the PSB BCMA RASO17 SRV Health Level Seven (HL7) server protocol is being disabled.**Corrective Action:**The error message is only intended to notify the BCMA software that the protocol is being disabled. BCMA will now validate the message and not display it to users.
 |

BCMA V. 3.0 and This Guide

|  |  |
| --- | --- |
| Benefits ofBCMA V. 3.0 (cont.) | 1. **Problem:** NOIS ISB-0104-31384When an IV medication order with an infusing bag is “Renewed,” the renewed order continues to display on the IV Medication Tab of the BCMA VDL until the infusing bag is “Completed,” even if the “Renewed” order’s Start Date/Time has expired.**Corrective Action:**When an IV medication order with an infusing bag is “Renewed,” the renewed order will continue to display on the IV Medication Tab of the BCMA VDL until the infusing bag is “Completed,” or until the Start Date/Time of the new order that was created during the renewal process. Once the new order is active, the infusing bag from the previous order will display on the BCMA VDL with the new order, along with any additional bags created from the new order. Any available bags from the previous order will display on the new order based on the IV Site Parameter settings in the GUI BCMA Site Parameters application.
 |

BCMA V. 3.0 and This Guide

|  |  |
| --- | --- |
| Benefits ofBCMA V. 3.0 (cont.)tip:You can double click on the PRN Effectiveness Activity in the BCMA Clinical Reminders marquee to document ALL PRN medication orders needing effectiveness documentation.j0255778tip:BCMA is designed to augment, not replace, the clinical judgment of the medication administrator, or clinician.j0255778 | This section provides an overview of the major changes in the Bar Code Medication Administration (BCMA) V. 3.0 software such as the new routines and files, Phase Release changes, and maintenance fixes. This version also includes enhancements, which are a direct result of feedback from the BCMA Workgroup and our many end users, and included in Phase Releases I-IV.Patient Transfer Notification MessageThe Patient Transfer Notification Information message displays when you open a patient’s record, or view the Unit Dose or the IVP/IVPB Medication Tab for the first time. It indicates that the patient has had a movement type (usually a transfer) within the Patient Transfer Notification Timeframe site-definable parameter, and the last action for the medication occurred before the movement, but still within the defined timeframe. You can define this site parameter, by division, with a minimum value of 2 and a maximum value of 99. The default is 72 hours. **Note:** The display of the message is dependent on the last action displayed in the “Last Action” column of the BCMA VDL. BCMA then evaluates the last action performed on a medication each time the Unit Dose or the IVP/IVPB Medication Tabs are refreshed.Documenting Fractional Dose OrdersYou can document Fractional Dose medication orders on the Unit Dose and the IVP/IVPB Medication Tabs. This functionality alerts you when dispensed drug dosages need to be administered to a patient in “fractional” doses so you can provide comments about this order type once administered. The Fractional Dose dialog box displays when the units per dose is fractional and *less than* 1.0. The Multiple/ Fractional Dose dialog box displays when the units per dose is *greater than* 1.0.**Note:** If you do not scan once for each unit listed in the Multiple/Fractional Dose dialog box, the Confirmation dialog box displays requesting that you confirm the actual total units administered.BCMA Clinical Reminders MarqueeLocated in the lower, right-hand corner of the BCMA VDL, this “marquee” identifies Pro Re Nata (PRN) medication orders needing effectiveness documentation. The setting is based on the PRN Documentation site-definable parameter, and applies to current admissions or to the site parameter timeframe (whichever is greater). Values can be set from 1-999, with 72 hours the default setting. A “mouse-over” list, in the PRN Effectiveness Activity area, provides the four most recent PRN orders that need comments. |

BCMA V. 3.0 and This Guide

|  |  |
| --- | --- |
| Benefits ofBCMA V. 3.0 (cont.) | PRN Documentation Site ParameterThe PRN Documentation site parameter lets you define the minimum number of hours from NOW that BCMA will search for PRN medication orders needing effectiveness comments. The four most recent PRN orders that need documentation display within the PRN Effectiveness mouse-over list in the “BCMA Clinical Reminders” marquee, located in the lower, right-hand corner of the BCMA VDL.The allowable entry for this parameter, definable by division, is a minimum value of 1 and a maximum value of 999. The default is 72 hours.Include Schedule Types Site ParameterYou can automatically display PRN medication orders when the BCMA VDL is first opened by selecting the PRN check box in the “Include Schedule Types” area of the GUI BCMA Site Parameters application. This parameter controls the default display of PRN medications on the BCMA Character-based User Interface (CHUI) Due List and the BCMA VDL **—** even if you change the Schedule Types or Medication Tab during a medication pass. Your medical center can choose to have the PRN Schedule Types display on the BCMA VDL by default, or to display PRN medications once a clinician selects the PRN Schedule Type check box on the BCMA VDL. All other Schedule Types will display by default and cannot be changed.Accessing PRN Effectiveness LogYou can quickly access the PRN Effectiveness Log dialog box by selecting a medication on the BCMA VDL, and then selecting the PRN Effectiveness command from the Right Click drop-down menu. The PRN Effectiveness Log displays the patient’s medication information at the top of the box, under the Selected Administration area, and all PRN medication administrations in the PRN List table. Once a medication is selected, the “Selected Administration” area of the dialog box populates with administration information. The Med History button on the dialog box displays the Medication History Report for the orderable item listed in the ”Selected Administration” area of the dialog box. |

BCMA V. 3.0 and This Guide

|  |  |
| --- | --- |
| Benefits ofBCMA V. 3.0 (cont.)tip:Discontinued and expired orders,with a Stop date/time greater than 72 hours from NOW, will not display on the VDL even if an infusing or stopped bag exists on the order.j0255778 | Schedule Type Indicator Alert LightsIn the Schedule Type area of the BCMA VDL, a **GREEN** “alert light” indicates that a medication order exists for the Schedule Type selected within the respective start/stop date and time selected on the BCMA VDL. If grayed out, then none exist.Medication Log Dialog BoxThe Medication Log dialog box includes the Vitals area, which displays the four previous vitals entries for each of the Vital signs listed in the area. The “+” (plus) sign, to the left of a Vital sign, expands the row to reveal additional entries. The “–” (minus) sign collapses the row to hide all, but the most recent entry.PRN Effectiveness Dialog BoxThe PRN Effectiveness dialog box includes the Vitals area, which displays the four previous vitals entries for each of the Vital signs listed in the area. The “+” (plus) sign, to the left of a Vital sign, expands the row to reveal additional entries. The “–” (minus) sign collapses the row to hide all, but the most recent entry.Scan IV Dialog BoxThe “Bag Information” title/area at the top of the Scan IV dialog box has been replaced with “IV Bag #.” BCMA populates this area with pertinent information about the IV bag selected on the BCMA VDL. The “Other Print Info” title has been replaced with “Order Changes,” which now displays changes to an IV order, which have an Infusing or Stopped IV bag.Bag Information Column on VDLThis new column on the BCMA VDL identifies an IV order that currently has an IV bag with a status of Infusing or Stopped. It also identifies orders that have changed since the Infusing or Stopped IV bag was first infused. |

BCMA V. 3.0 and This Guide

|  |  |
| --- | --- |
| Benefits ofBCMA V. 3.0 (cont.) | Report PrintingHere’s the changes to the report printing functionality in BCMA V. 3.0:* **Medication Administration History (MAH) Report:** The Date column lists three asterisks (\*\*\*) to indicate that a medication is notdue. This information is also noted in the Legend at the bottom of the MAH Report. The report also includes information about when an order is placed “On Hold” and taken “Off Hold” by a provider, and the order Start and Stop Date/Time for the medication.
* **Medication Variance Report:** Provides “exceptions” (variances) to the medication administration process. It also lists “event” information within a selected date range, such as the type and number of events, and the total percentage of events that occurred. A variance preceded by a minus sign (such as –24) indicates the number of minutes that a medication was given before the administration time.
* **Cumulative Vitals/Measurement Report:** Lists a patient’s vitals from the Vitals package, along with their demographics and hospital location information. You cannot print this report by ward.
* **Ward-Specific Reports:** Simply click **cancel** at the Patient Lookup dialog box to access the Menu Bar — without opening a patient record — and print ward-specific reports only, except for the Cumulative Vitals/Measurement Report. A patient’s file must be opened to access patient-specific reports.
* **Missed Medications Report:** Indicates when a medication order is placed “On Hold” and taken “Off Hold” in CPRS or Inpatient Medications V. 5.0. The Hold information is provided below the medication information on the report, and only applies to administrations due within the Hold timeframe. The “Order Num” column on the report lists the actual order number and order type (i.e., Unit Dose or IV). This information is quite helpful when troubleshooting problems with BCMA.
* **CHUI Missing Dose Report:** Changed the line item “Dosage Schedule” on the BCMA CHUI Missing Dose Report to “Schedule” to coincide with the Missing DoseE-mail Notification change described on the next page.
 |

BCMA V. 3.0 and This Guide

|  |  |
| --- | --- |
| Benefits ofBCMA V. 3.0 (cont.) | HL7 MessagingBCMA V. 3.0 supports “Health Level Seven (HL7),” a standard package (**V***IST***A** Messaging) used with M-based applications for conducting HL7 transactions. This package provides the facilities to create, transmit, and receive HL7 messages over a variety of transport layers. BCMA onlyexports HL7 messages.Missing Dose E-Mail NotificationThe e-mail notification that is sent from BCMA to the Pharmacy, when you submit a Missing Dose Request, now includes “Schedule” information. Documenting PRN Pain ScoresWith BCMA V. 3.0, you can perform the following tasks with regards to documenting PRN pain scores:* **Define Items:** In the “Reason Medication Given PRN” default Answer Lists of the GUI BCMA Site Parameters application you can identify those items that will require the documentation of a pain score within BCMA. The pain score will be documented and stored in the Vitals package.
* **Select a Pain Score:** When documenting an administration for a PRN medication, you can select a pain score from a pre-defined list.
* **Access a Pain Score:** When documenting the effectiveness for a PRN medication, you can access pain score information for the patient.
 |

BCMA V. 3.0 and This Guide

|  |  |
| --- | --- |
| Benefits ofBCMA V. 3.0 (cont.) | Administering a Multiple Dose OrderIf you do not scan once for each Unit Dose or IVP medication listed in the Multiple Dose dialog box, BCMA displays the Confirmation dialog box informing you to scan additional units. The Multiple Dose dialog box retains the data that you entered before receiving the message.Administering a PRN OrderIn the Medication Log dialog box, you can select the patient’s pain score, between 0 and 10 or 99, with “0” being No Pain, “10” the Worst Imaginable, and “99” for “Unable to Respond.”Recording the Effectiveness of a PRN MedicationIn the PRN Effectiveness Log dialog box, you can select the patient’s pain score, between 0 and 10 or 99, with “0” being No Pain, “10” the Worst Imaginable, and “99” for “Unable to Respond.”Creating Default Answers Lists In the GUI BCMA Site Parameters application, the Attribute column is available only when you choose the Default Answer Lists Tab and select the “Reason Medication Given PRN” list. This column identifies that a Pain Score is required from the patient when a clinician administers a specific medication.When you select the “Requires Pain Score” check box when adding or renaming a “Reason Medication Given PRN” item, you must choose a pain score in the BCMA Medication Log and PRN Effectiveness dialog boxes when administering a medication. |

BCMA V. 3.0 and This Guide

|  |  |
| --- | --- |
| Benefits ofThis Guide | Preparing your site for the installation and implementation ofBCMA V. 3.0 helps to ensure a smooth integration. This Installation Guide is designed to help you do just that. It includes detailed information such as system requirements; installation time estimates and instructions; and procedures that will get you up and running quickly with BCMA V. 3.0.Our Target AudienceWe have developed this guide for the following individuals, who are responsible for installing, supporting, maintaining, and testing this package.* Development Engineering
* Information Resources Management (IRM)
* Clinical Application Coordinator (CAC) – called Applications Package Coordinator (ADPAC) at some sites
* Enterprise **V***IST***A** Support (EVS)
* Software Quality Assurance (SQA)
 |
|  |  |
| Other Sourcesof Informationtip:Bookmark these sites for future reference.j0255778tip:Bookmark these sites for future reference.j0255778 | Refer to the Web sites listed below when you want to receive more background and technical information about BCMA V. 3.0, and to download this manual and related documentation.Background/Technical InformationFrom your Intranet, enter REDACTED in the Address field to access the BCMA Main Web page.This Manual and Related DocumentationFrom your Intranet, enter <http://www.va.gov/vdl> in the Address field to access this manual, and those listed below, from the **V***IST***A** Documentation Library (VDL).* Technical Manual/Security Guide
* GUI User Manual
* Nursing CHUI User Manual
* Pharmacy CHUI User Manual
* Manager’s User Manual
 |

BCMA V. 3.0 and This Guide

|  |  |
| --- | --- |
| Documentation Retrieval Processtip:Bookmark these sites for future reference.j0255778tip:Bookmark these sites for future reference.j0255778 | Your site can retrieve the BCMA V. 3.0 documentation listed below from the following FTP addresses. The preferred method is to “FTP” the files from REDACTED. This location automatically transmits files from the first available FTP Server to the appropriate directory on your system. (See the order listed below under the FTP Address column).**Note:** If you prefer, you can retrieve the software *directly* from one of the FTP Servers, listed below, under the FTP Address column. |

**Example: FTP Addresses Available for Downloading
BCMA V. 3.0 Documentation**

|  |  |  |
| --- | --- | --- |
| **OI Field Office** | **FTP Address** | **Directory** |
| REDACTED | REDACTED | REDACTED |
| REDACTED | REDACTED | REDACTED |
| REDACTED | REDACTED | REDACTED |

**Example: BCMA V. 3.0 Documentation and Related File names**

|  |  |
| --- | --- |
| **BCMA V. 3.0 Documentation** | **Documentation File name** |
| Installation Guide | PSB\_3\_IG\_R0204.PDF |
| Technical Manual/Security Guide | PSB\_3\_TM\_R0204.PDF |
| GUI User Manual | PSB\_3\_UM\_Chapters 1 through 4\_R0204.PDFPSB\_3\_UM\_Chapters 5 through 8\_R0204.PDFPSB\_3\_UM\_Appendix A\_(FAQs)\_R0204.PDFPSB\_3\_UM\_Appendix B\_(Index)\_R0204.PDF |
| Nursing CHUI User Manual | PSB\_3\_UM\_NURSE\_CHUI\_R0204.PDF |
| Pharmacy CHUI User Manual | PSB\_3\_UM\_PHAR\_CHUI\_R0204.PDF |
| Manager’s User Manual | PSB\_3\_UM\_MGR\_R0204.PDF |

BCMA V. 3.0 and This Guide

|  |  |
| --- | --- |
| Conventions Used in This Guidetip:In a CHUI environment, when you press **enter**, instead of typing a response, the system accepts the default value shown to the left of the double slash (//) at a prompt or a field.j0255778tip:In a CHUI environment, when you press the ENTER key, instead of typing a response, the system accepts the default value shown to the left of the double slash (//) at a prompt or field.j0255778tip:In a CHUI environment, when you press the ENTER key, instead of typing a response, the system accepts the default value shown to the left of the double slash (//) at a prompt or field.j0255778 | Before installing BCMA V. 3.0, review this section to learn the many conventions used throughout this guide. * **Keyboard Responses:** Keys provided in **boldface**, within the steps, help you quickly identify what to press on your keyboard to perform an action. See the examples provided below.
* **Within the Steps:** At the “Select Kernel Installation & Distribution System Option:” prompt, type **INSTALL**, and then press **enter**.
* **Within Screen Captures:** Text in **boldface**, centered between arrows on screen captures, identifies the key you must press for the system to capture your response or to move the cursor to the next field. See the following example.

DEVICE FOR QUEUED JOB OUTPUT: **<Enter>*** **Mouse Responses:** Buttons provided in **boldface**, within the steps, indicate what you should click on your computer screen using the mouse. For example, when you see **next, yes/no,** or **ok** in the steps, click the appropriate button on your computer screen.
* **User Responses:** Information presented in **boldface**, within steps or shaded screen captures, indicate what you should “type” (enter) onto your computer screen. See the examples provided below.
* **Within the Steps:** At the “Select OPTION NAME:” prompt, type **XPD MAIN** and then press **enter**.
* **Within Screen Captures:** See the following example.

 RESCHEDULING FREQUENCY: **1M*** **Screen Captures:** Provide “shaded” examples of whatyou will see on your computer screen, and possible user responses.
* **Notes:** Provided within the steps, describe exceptions or special cases about the information presented. They reflect the experience of our staff, developers, and testers.
 |

BCMA V. 3.0 and This Guide

|  |  |
| --- | --- |
| Conventions Used in This Guide (cont.)tip:In a CHUI environment, you can exit a menu option by typing a caret (^), then pressing **enter**. A caret is sometimes called Up-Arrow.j0255778 | * **Tips:** Located in the left margin, these helpful hints are designed to help you work more efficiently with BCMA V. 3.0.
* **Menu Options:** When provided in *italics*, identifies a menu option. When provided in **boldface**, ALL CAPS, identifies the letters that you should type onto your computer screen, before pressing **enter**. The system then goes directly to the menu option. (**Note:** The letters do not have to be entered as capital letters, even though they are provided within the steps in this format.) See the examples provided below.
* **Italicized:** Use the Kernel *First Line Routine Print* [XU FIRST LINE PRINT] option to print a list containing the first line of every PSB routine.
* **Capitalized:** At the “Taskman Management Option:” prompt, type **SCHED**ule/Unschedule Options, and then press **enter**.
 |

BCMA V. 3.0 and This Guide

|  |  |
| --- | --- |
| ObtainingOn-line Help | On-line help is designed right into the Graphical User Interface (GUI) and Character-based User Interface (CHUI) versions of BCMA V. 3.0, making it quick and easy for you to get answers to your questions. Here’s how to access help in both versions of BCMA V. 3.0:* **GUI BCMA:** Provides context-sensitive, on-line help and the Help menu.
* **Context-Sensitive Help:** Place your “focus” on a feature, button, or Tab on the BCMA VDL, using the **tab** key, and then press **f1** to receive help specific to that area of the BCMA VDL. In the case of a command, first highlight it in the Menu Bar or Right Click drop-down menu, and then press **f1**.
* **Help Menu:** Open the Help menu, and then choose the Contents and Index command to receive help for every feature in GUI BCMA V. 3.0.
* **CHUI BCMA:** Lets you enter up to two question marks at any prompt to receive on-line help.
* **One Question Mark:** Provides a brief statement related to the prompt.
* **Two Question Marks:** Displays more detailed information about the prompt, plus any hidden actions.
 |
|  |  |
| LocatingDetailed Listings | You can obtain andprint listings about BCMA V. 3.0 routines, and Data Dictionaries using the information provided below.RoutinesUse the Kernel routine XINDEX to produce detailed listings of routines. Use the Kernel *First Line Routine Print* [XU FIRST LINE PRINT] option to print a list containing the first line of every PSB routine.Data DictionariesYou can use the VA FileMan *List File Attributes* [DILIST] option, under the *Data Dictionary Utilities* [DI DDU] option, to print the Dictionaries. |

# Pre-Installation Information

|  |  |
| --- | --- |
| Minimum Required Packages | Before installing BCMA V. 3.0, make sure that your system includes the following Department of Veterans Affairs (VA) software packages and versions (those listed or higher).  |

Example: Minimum Required Packages and Versions

|  |  |
| --- | --- |
| Package | Minimum Version Needed |
| Inpatient Medications | 5.0 |
| Kernel | 8.0 |
| MailMan | 8.0 |
| Nursing | 4.0 |
| Order Entry/Results Reporting | 3.0 |
| Pharmacy Data Management | 1.0 |
| RPC Broker (32-bit) | 1.1 |
| Toolkit | 7.3 |
| VA FileMan | 22.0 |
| Vitals/Measurements | 5.0 |

|  |  |
| --- | --- |
| Installation Time Estimatesimportant:You should install and test BCMA in your test accounts ***before***installing in your production accounts.j0255778 | On average, it takes approximately twominutes to install BCMAV. 3.0. This estimate was provided by a few of our BCMA V. 3.0 Beta Test sites. Actual times may vary, depending on how your site is using its’ system resources.Suggested time to install: non-peak requirement hours. During the install process, PC Client users should not be accessing the Client Software. |

Pre-Installation Information

|  |  |
| --- | --- |
| Resource Requirementstip:The approximate size for ^PSB was calculated using a “normal” medication pass for a Unit Dose and an IV medication order. This is only an estimated number; it serves as the “mean.”j0255778 | This section summarizes the (approximate) number of resources required to install BCMA V. 3.0.* Routines 60
* Globals 1 (^PSB)
* Files 5 (53.66-53.79)
* ^PSB Size Unit Dose = 300 x # of Medications(in bytes) Administered IV = 2100 x # of IV Bags Administered
* FTEE Support .2
* FTEE Maintenance .2

Response Time MonitorBCMA V. 3.0 does not include Response Time Monitor hooks.Laptops and Bar Code ScannersThe approximate requirements for laptops and bar code scanners depend on the number of Inpatient areas, at your site, that use BCMA V. 3.0 for administering activemedication orders. The BCMA Development Team recommends that your site have a minimum of three laptops and three scanners for each ward.PrintersYour site should provide printers for creating patient wristbands and medication bar code labels, and for handling Missing Dose Requests sent from BCMA V. 3.0 to the Pharmacy.Unit Dose Label Printer DevicesBCMA V. 3.0 includes the *Label print* [PSBO BL] option for printing individual or batch Unit Dose bar code labels. It is specifically coded to the Zebra-brand printers using the Zebra Programming Language (ZPL). Model 105SE was used in the development of the labels. Routine PSBO BL uses site-specific printers or terminals to produce labels.IV Label Printer DevicesInpatient Medications V. 5.0 provides a menu option for printing individual or batch IV bar code labels. See the section “Interfacing with the Bar Code Label Printer” in the *Inpatient Medications V. 5.0 Technical Manual/Security Guide* for detailed setup information.  |

Pre-Installation Information

|  |  |
| --- | --- |
| Client PC Setup Requirements | Once all BCMA V. 3.0 files are installed, make sure that every Client PC includes the minimum system *before* users run BCMA V. 3.0 from it. BCMA must be installed via an account that has Administrative privileges. For specific Client PC Setup Requirements, see the “VA Standard Desktop Configurations” link below, which provides the current corporate software and hardware configurations per VA Directive 6401.* REDACTED
 |
|  |  |
| Files Required to Run BCMA V. 3.0tip:The namespace for the BCMA package is PSB and the primary globalis ^PSB.j0255778 | BCMA V. 3.0 uses the following files installed on the **V***IST***A** Server. “Journaling” is recommended.* ^PSB (53.66, BCMA IV Parameters
* ^PSB (53.68, BCMA Missing Dose Request
* ^PSB (53.69, BCMA Report Request
* ^PSB (53.78, BCMA Medication Variance Log
* ^PSB (53.79, BCMA Medication Log

Note: You can learn more about these files by generating a list with file attributes using VA FileMan. |

Pre-Installation Information

|  |  |
| --- | --- |
| Routines Installed | Review the listing below to learn the routines installed on to your site’s **V***IST***A** Server during the installation of BCMA V. 3.0. The first line of each routine briefly describes its general function.**Note:** You can use the *Kernel First Line Routine Print* [XU FIRST LINE PRINT] option to print a list containing the first line of each PSB routine.Routine MappingAt this time, we do *not* offer any recommendations for routine mapping. However, if you choose to map the BCMA V. 3.0 package routines, you will need to bring your system down, and then restart it to load the new routines into memory. |

Example: BCMA V. 3.0 Routines Installed on to V*IST*A Server

|  |
| --- |
| PSBALL PSBAPIPM PSBCHIVH PSBCHKIV PSBMD PSBML PSBML1 PSBMLENPSBMLEN1 PSBMLHS PSBMLTS PSBMLU PSBMLVAL PSBO PSBO1 PSBOALPSBOBL PSBODL PSBODL1 PSBODO PSBOHDR PSBOMD PSBOMH PSBOMH1PSBOMH2 PSBOML PSBOMM PSBOMV PSBOPE PSBOPI PSBOPM PSBOVTPSBOWA PSBPAR PSBPARIV PSBPOIV PSBPRN PSBRPC PSBRPC1 PSBRPC2PSBRPC3 PSBRPCMO PSBRPCXM PSBSAGG PSBSVHL7 PSBUTL PSBVAR PSBVDLIVPSBVDLPA PSBVDLPB PSBVDLTB PSBVDLU1 PSBVDLU2 PSBVDLU3 PSBVDLUD PSBVDLVLPSBVITFL PSBVT PSBVT1 PSBXMRG60 routines |

Pre-Installation Information

|  |  |
| --- | --- |
| Routines with Related Checksums | This section lists the routines and related checksums for BCMAV. 3.0 provided during the installation process. |

Example: BCMA V. 3.0 Routines with Related Checksums

Select BUILD NAME: PSB 3.0 BAR CODE MED ADMIN

PSBALL value = 1475151

PSBAPIPM value = 9031085

PSBCHIVH value = 1166996

PSBCHKIV value = 35513271

PSBMD value = 17319681

PSBML value = 23421797

PSBML1 value = 7074072

PSBMLEN value = 18077803

PSBMLEN1 value = 9220985

PSBMLHS value = 2525483

PSBMLTS value = 8100734

PSBMLU value = 1498988

PSBMLVAL value = 9734944

PSBO value = 17926200

PSBO1 value = 2876667

PSBOAL value = 1806300

PSBOBL value = 4045534

PSBODL value = 16589922

PSBODL1 value = 8836828

PSBODO value = 2948451

PSBOHDR value = 5286664

PSBOMD value = 6143174

PSBOMH value = 20105393

PSBOMH1 value = 20721307

PSBOMH2 value = 9443664

PSBOML value = 10399745

PSBOMM value = 21442785

PSBOMV value = 13276146

PSBOPE value = 7022505

PSBOPI value = 288600

PSBOPM value = 4855752

PSBOVT value = 790819

PSBOWA value = 13904863

PSBPAR value = 6032995

PSBPARIV value = 16437954

PSBPOIV value = 24363099

PSBPRN value = 7079605

PSBRPC value = 10743383

PSBRPC1 value = 5473533

PSBRPC2 value = 20110546

PSBRPC3 value = 194738

Pre-Installation Information

Example: BCMA V. 3.0 Routines with Related Checksums (cont.)

PSBRPCMO value = 18080428

PSBRPCXM value = 2728593

PSBSAGG value = 1431404

PSBSVHL7 value = 16217830

PSBUTL value = 14185290

PSBVAR value = 4760179

PSBVDLIV value = 17858201

PSBVDLPA value = 4059667

PSBVDLPB value = 19523684

PSBVDLTB value = 3557813

PSBVDLU1 value = 18022165

PSBVDLU2 value = 4610568

PSBVDLU3 value = 3001261

PSBVDLUD value = 18568646

PSBVDLVL value = 23162182

PSBVITFL value = 2483832

PSBVT value = 22976876

PSBVT1 value = 767427

PSBXMRG value = 1576759

# Installation Information

|  |  |
| --- | --- |
| V*IST*A Server Installation Instructionstip:Performing the steps in this section will help to ensure that GUI BCMAruns smoothlyfrom a Client PC. j0255778tip:See Attachment A to view a sample of a KIDS load and installation. j0255778important:You should install and test BCMA in your test accounts ***before***installing in your production accounts.j0255778 | Perform the steps provided below to download BCMA V. 3.0 from an FTP Server. Then you will be ready to use this section for loading the Kernel Installation & Distribution System (KIDS) Distribution file and the Broker Server file, and for installing BCMA V. 3.0 on to the **V***IST***A** Server. **Attention:** BCMA V. 3.0 includes a new GUI executable file. Installation of this GUI is NOT required immediately after the KIDS install for the software to function. The installation process will make significant changes to routines, files, and files within the BCMAV. 3.0 application. Review the bulleted list below, taken from the Build description, for more information.* Prior clients compatible with BCMA V. 3.0: 2.0.36.14
* Client can be copied instead of installed: Yes

Task 1: Download BCMA V. 3.0 SoftwareUse the following information to download BCMA V. 3.0 from an FTP Server. 1. Download the GUI BCMA file PSB3\_0.exe, the Host File PSB\_3\_0.KID from an FTP Server using an address listed in the table below.
* The preferred method is to “FTP” the files from REDACTED This location automatically transmits files from the *first* available FTP Server. (See the order listed below under the FTP Address column).
* .EXE or .PDF files need to be FTP in BINARY.
* KIDS Build needs to be FTP in ASCII.

**Note:** If you prefer, you can retrieve the software *directly* from one of the FTP Servers, listed below, under the FTP Address column.1. Move the files to the appropriate directory on your system.
 |

Example: FTP Addresses Available for Downloading BCMA V. 3.0 Software

|  |  |  |
| --- | --- | --- |
| OI Field Office | FTP Address | Directory |
| REDACTED | REDACTED | REDACTED |
| REDACTED | REDACTED | REDACTED |
| REDACTED | REDACTED | REDACTED |

#

Installation Information

|  |  |
| --- | --- |
| V*IST*A Server Installation Instructions (cont.) | Task 2: Load the KIDS Distribution FilePerform the steps listed below to load the KIDS Distribution file.1. Sign in to the UCI where the KIDS Distribution file will be loaded and BCMA V. 3.0 will be installed.
2. At the “Select OPTION NAME:” prompt, type **XPD MAIN**, and then press **enter**.
3. At the “Select Kernel Installation & Distribution System Option:” prompt, type **INSTALL**ation, and then press **enter**.
4. At the “Select Installation Option:” prompt, type **Load a Distribution,** and then press **enter** to prepare for loading the KIDS Distribution file.
5. At the “Enter a Host File:” prompt, type **the directory where you have stored the Host File**, followed by **PSB\_3\_0.KID**. Then press **enter**.
6. At the “Want to Continue with Load YES//?” prompt, press **enter**. The system then loads the file to this location.

Task 3: Install BCMA V. 3.0Now you are ready to install BCMA V. 3.0 on to the **V***IST***A** Server. Suggested time to install: non-peak requirement hours. During the install process, PC Client users should not be accessing the Client Software.Note: You should perform step #1 listed below *now* if you are planning to install BCMA V. 3.0 immediately. However, if you are installing the application at another time, ask users to log off your system at that time.1. From the Facility Tab of the GUI BCMA Site Parameters application, take BCMA users offline.
2. Request that all BCMA users log off BCMA.
3. Review mapped sets for PSB\* namespaces.
* If the routines are mapped, remove them from the mapped set at this time.
1. Backup your system. This step is optional, but recommended.
2. At the “Select INSTALL NAME:” prompt, type PSB 3.0 and then press **enter** to install BCMA V. 3.0. This Build provides all of the routines and files necessary for BCMA V. 3.0.
 |

Installation Information

|  |  |
| --- | --- |
| V*IST*A Server Installation Instructions (cont.) | Task 3: Install BCMA V. 3.0 (cont.)1. At the “Want KIDS to Rebuild Menu Trees Upon Completion of Install? YES//” prompt, type **NO**, and then press **enter**.
2. At the “Want KIDS to INHIBIT LOGONs during the install? YES//” prompt, type **NO**, and then press **enter**.
3. At the “Want to DISABLE Scheduled Options, Menu Options, and Protocols? YES//” prompt, type **NO**, and then press **enter**.
4. At the “DEVICE:” prompt, press **enter** to use the default device HOME (the screen) for printing the Installation message. If you want to print a hard copy, enter your site printer, and then press **enter.**
5. If routines were unmapped as part of the installation process, return them to the mapped set once the installation ofBCMA V. 3.0 is completed.
6. From the Facility Tab of the GUI BCMA Site Parameters application, place BCMA V. 3.0 back on-line.

Additional Preparation for BCMA V. 3.0Now you are ready to perform the steps listed below to further prepare your site and staff for using BCMA V. 3.0.1. If you are a Micronectics Standard MUMPS (MSM) site, move the PSB routines only, to all nodes.
2. Assign the following security keys to appropriate site personnel.
* **PSB MANAGER** – designates the holder as a manager
* **PSB INSTRUCTOR** – designates the holder as a nursing instructor supervising student nurses
* **PSB STUDENT** – designates the holder as a student nurse, requiring that an instructor also sign on to BCMA V. 3.0at the same time
* **PSB CPRS MED BUTTON** – designates the holder as a nurse who can document administered verbal- and phone-type STAT and NOW orders using the CPRS Med Order Button on the BCMA V. 3.0 VDL
 |

#

# Working with GUI BCMA V. 3.0

|  |  |
| --- | --- |
| Client PC Setup Requirements | Once all BCMA V. 3.0 files are installed, make sure that every Client PC includes the minimum system configuration *before* users run BCMA V. 3.0 from it. BCMA must be installed via an account that has Administrative privileges. For specific Client PC Setup Requirements, see the “VA Standard Desktop Configurations” link below, which provides the current corporate software and hardware configurations per VA Directive 6401.REDACTED |
|  |  |
| Client Distribution Files | This section lists the Client files distributed during the installation of BCMA V. 3.0. **Note: the file list has been updated to reflect current file versions releasing with PSB\*3.0\*123.** |

Example: Client Files Distributed During BCMA V. 3.0 Installation

|  |  |  |  |
| --- | --- | --- | --- |
| File names | Description | File Version | Bytes |
| BCMA.exe | Main BCMA application | 3.0.123.3 | 8,120 |
| BCMA.chm | BCMA help file |  | 1,180 |
| OrderCom.dll | CPRS Med Order Button, Dynamic Link Library (DLL) | 2.0.18.3 | 4,724 |
| BCMApar.exe | GUI BCMA Site Parameters Application | 3.0.123.3 | 5,664 |
| BCMApar.chm | Site Parameter help file |  | 161 |
| ReadMe.txt | Supplementary Information |  | 5 |

Note: The BCMAOrderCom.dll was replaced with the OrderCom.dll file released in PSB\*3.0\*96. With the release of PSB\*3.0\*96 you can remove all instances of the BCMAOrderCom.dll file. Also, ROBOEX32.DLL is no longer needed or distributed.

Working with GUI BCMA V. 3.0

|  |  |
| --- | --- |
| Standard Installation Procedure for GUI BCMA V. 3.0tip:You can useBCMA V. 3.0 to upgrade an earlier version of BCMA,or you can install BCMA V. 3.0 without previous versions being installed.j0255778 | Use the instructions listed below to install the GUI version ofBCMA V. 3.0, on a Client PC. To install GUI BCMA V. 3.0 on a Client PC1. Locate the directory where you downloaded the GUI BCMAV. 3.0 file PSB\_3\_0P123 via FTP, and then double click on the file to launch the InstallShield Wizard.
2. Click **yes** at the message, "Would you like to install BCMA?”
3. At the InstallShield Wizard Welcome screen, click **next**.
4. Read the contents of the BCMA Installation screen, and then click **next**.
5. Click **next** at the Choose Destination Location screen.
* Click **browse** if you want to locate another folder to replace the default destination folder. Once located and selected, click **next** to proceed with the installation process.
1. At the Setup Type screen, select one of the following choices, and then click **next** to continue with the installation process. “Typical” is the default installation.
* **Typical** – Installs only the BCMA Client program, which is necessary for using BCMA V. 3.0 to perform the medication administration process.
* **Full** – Installs the BCMA Client program, and the GUI BCMA Site Parameters application.
* **Custom** – Lets you select which programs (i.e., BCMA Client program or GUI BCMA Site Parameters application) that you want to install.
1. At the InstallShield Wizard Complete screen, click **finish** to complete the BCMA installation process. BCMA V. 3.0 is now installed on to the PC.
 |

Working with GUI BCMA V. 3.0

|  |  |
| --- | --- |
| Working with the Hosts File on the Client PCtip:You *must* have at least one space between the address and the name. Do *not* put any spaces inthe name.j0255778tip:Users *must* have FULL read/write access to the BCMA directory on the Client PC that they’re using.j0255778 | Make sure that every Client PC has a link established between the Client PC and the **V***IST***A** Server via the Hosts file on the PC — *before* running GUI BCMA V. 3.0 from a Client PC. Then you can set up the Optional Command Line Parameters using the table provided in the next section.Where your Hosts file (no extension) is located, depends on your system. For example: * **Microsoft XP or 2000 operating system** – C:\WinNt\System32\Drivers\Etc.
* If No Hosts File Exists

If the Hosts file does not exist, create one. (Your system may already contain a sample file called “hosts.sam.”) If you create the file using Notepad, it will automatically save the file with a .txt extension. You can use Microsoft Windows Explorer to rename the file without an extension. * If the Hosts File Exists

If the Hosts file already exists, donotdelete anything. Just add the new information (i.e., the address and the name) at the end of the file. See the examples provided below. * **If a user only needs access to one BCMA Server and the ServerPort is 9200,** add one line to the Hosts file. Use the IP address provided by your Server Administrator. See the example provided below.
* 152.111.222.333 BrokerServer
* **If the user only needs to access one BCMA Server *and* the ServerPort is *not* 9200,** add one line to the Hosts file as shown in the example provided above. Then use the table in the next section to set up the Optional Command Line Parameters.
* **If the user needs to access multiple BCMA Servers and/or the ServerPort is *not* 9200,** add the BCMA Server names to the Hosts file. (The names can be anything you like.) See the examples listed below. Then use the table in the next section to set up the Optional Command Line Parameters.
* 152.111.222.333 BrokerServer1
* 152.222.333.444 BrokerServer2
 |

#

Working with GUI BCMA V. 3.0

|  |  |
| --- | --- |
| Setting up Optional Command Line Parameters | Use the table provided below to set up the Optional Command Line Parameters. The order that you set up each Parameter is up to your site. However, each Parameter must be continuous, without any spaces. **Note:** If Parameters “S” and “P” are set, they must both be present,or the Client PC will ignore them.  |

Example: Set up for Optional Command Line Parameters

|  |  |  |
| --- | --- | --- |
| Parameter | Example(default) | Description |
| S= | S=BrokerServer | The name of the BCMA Broker Server, as defined in the Hosts file. The default is “BrokerServer.” |
| P= | P=9200 | The server port used by the BCMA Broker Server. The default is “9200.” |
| L= | L=C:\Temp | The DOS path location for the BCMA Error Log file. Any DOS path will work. The default is “C:\Temp.” |
| T= | T=300 | RPC Broker TimeOut in seconds. This is the amount of time that BCMA V. 3.0 will wait for a response from an RPC on V*IST*A. If it is not defined, the default value is five minutes. The minimum value is 30 seconds; anything less is ignored. If the V*IST*A System's CPU utilization is near 100 percent, and frequent timeouts occur in theGUI version of BCMA V. 3.0, you can increase this value. NOTE: The higher the value, the longer BCMA V. 3.0 will appear to hang until the RPC Broker call is complete. |
| /NOLOGFILE |  | This parameter disables the Error Log. |
| /DEBUG |  | This parameter turns on (displays) the BCMA Debug screens. |
| -S –A –S |  | Silent install. These command line parameters only work on the distribution file. For example: PSB2\_0P24.exe -s -a –sThe silent install will only install the GUI BCMA application, and will not install the GUI BCMA Site Parameters application. At this time, a silent un-install does not exist. |

# Working with the Monthly SAGG Report

|  |  |
| --- | --- |
| Setting up the Monthly Batch Jobtip:You can use FORUM to view your monthly SAGG Report.j0255778tip:In step #7, ### is the numberof the entry.j0255778tip:See the next page to view the set upof a monthlySAGG Report.j0255778 | Use the steps listed below to set up your system to run the Monthly Statistical Analysis of Global Growth (SAGG) Report. **Note:** You do notneed to perform the steps listed below if you have already set up the Monthly SAGG Report. To set up the monthly batch job1. At the Programmer’s prompt, type **D ^XUP**, and then press **enter** to access the menu option for setting up your Monthly SAGG Report.
2. At the “Select OPTION NAME:” prompt, type **EVE**, and then press **enter**.
3. From the list of choices, select Systems Manager Menu, and then press **enter**.
4. At the “Select Systems Manager Menu Option:” prompt, type **TASK**man Management,and then press **enter.**
5. At the “Select Taskman Management Option:” prompt, type **SCHED**ule/Unschedule Options, and then press **enter**.
6. At the “Select OPTION schedule or reschedule:” prompt, type **PSB SAGG MONTHLY REPORT**, and then press **enter**.
7. At the “Are you adding ‘PSB SAGG MONTHLY REPORT’ as a new OPTION SCHEDULING (the ###)? No//” prompt, type **Yes**, and then press **enter**. The Edit Option Schedule screen displays.
8. At the “QUEUED TO RUN AT WHAT TIME:” prompt, type a **date and time** **when you want the report to run**, in a VA FileMan format. Then press **enter** to move to the next prompt.
9. At the “DEVICE FOR QUEUED JOB OUTPUT:” prompt, press **enter** (leave this prompt blank).
10. At the “QUEUED TO RUN ON VOLUME SET:” prompt, type **the volume set (CPU)** to use for running the monthly batch job. Then press **enter** to move to the next prompt.
11. At the “RESCHEDULING FREQUENCY:” prompt, type **1M** to run the report on a monthly basis. Then press **enter** to move to the next prompt.
12. At the “TASK PARAMETERS:” prompt, press **enter** (leave this prompt blank).
13. At the “SPECIAL QUEUEING:” prompt, press **enter** (leave this prompt blank).
14. At the “COMMAND:” prompt, type **S** to save the settings, and then press **enter**. Your report will print on the same day and time each month (until you specify otherwise).
15. At the “COMMAND:” prompt, type **E** to exit the Edit Option Schedule screen.
 |

#

Working with the Monthly SAGG Report

|  |  |
| --- | --- |
| Setting up the Monthly Batch Job (cont.) | The following example illustrates the set up process for running the SAGG Monthly Report at your site. |

Example: Set up for SAGG Monthly Report

>**D ^XUP**

Setting up programmer environment

Terminal Type set to: C-VT320

Select OPTION NAME: **EVE**

 1 EVE Systems Manager Menu

 2 EVENT CAPTURE DATA ENTRY ECENTER Event Capture Data Entry

 3 EVENT CAPTURE MANAGEMENT MENU ECMGR Event Capture Management Menu

 4 EVENT CAPTURE MENU ECMENU Event Capture Menu

 5 EVENT CAPTURE ONLINE DOCUMENTA ECDSONL Event Capture Online Documentation

Press <RETURN> to see more, '^' to exit this list, OR

CHOOSE 1-5: 1 EVE Systems Manager Menu

Select Systems Manager Menu Option: **TASK**man Management

Select Taskman Management Option: **SCHED**ule/Unschedule Options

Select OPTION to schedule or reschedule: **PSB SAGG MONTHLY REPORT** Monthly SAGG Report

 ...OK? Yes// **<Enter>**

Working with the Monthly SAGG Report

|  |  |
| --- | --- |
| Setting up the Monthly Batch Job (cont.) | The example provided below illustrates the prompts (fields) to complete on the Edit Option Schedule screen for running the PSB SAGG Monthly Report at your site. |

Example: Set up for SAGG Monthly Report (cont.)

 Edit Option Schedule

 Option Name: PSB SAGG MONTHLY REPORT

 Menu Text: Monthly SAGG Report TASK ID:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 QUEUED TO RUN AT WHAT TIME: **<Date, time to run the report>**

DEVICE FOR QUEUED JOB OUTPUT: **<Enter>**

 QUEUED TO RUN ON VOLUME SET: **<Volume set (CPU)>**

 RESCHEDULING FREQUENCY: **1M**

 TASK PARAMETERS: **<Enter>**

 SPECIAL QUEUEING: **<Enter>**

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Exit Save Next Page Refresh

Enter a command or '^' followed by a caption to jump to a specific field.

COMMAND: **S** Press <PF1>H for help Insert

COMMAND: **E** Press <PF1>H for help Insert

# Glossary

|  |  |
| --- | --- |
| Learning BCMAV. 3.0 Lingo | The alphabetical listing, in this section, is designed to familiarize you with the many acronyms and terms used throughout this guide. |

Example: Alphabetical Listing of BCMA V. 3.0 Acronyms and Terms

|  |  |
| --- | --- |
| Acronym/Term | Definition |
| Broker Server | The M portion of the RPC Broker within the VA’s Veterans Health Information Systems and Technology Architecture (**V***IST***A**) environment. |
| CHUI | **Ch**aracter-based **U**ser **I**nterface. |
| Client | An architecture in which one computer can get information from another. The Client is the computer that asks for access to data, software, or services. |
| CPRS | **C**omputerized **P**atient **R**ecord **S**ystem. A **V***IST***A** software application that allows users to enter patient orders into different software packages from a single application. All pending orders that appear in the Unit Dose and IV packages are initially entered through the CPRS package. Clinicians, Managers, Quality Assurance Staff, and Researchers use this integrated record system. |
| Data Dictionary | Also called “DD,” the dictionary that contains file attributes. |
| FileMan | The **V***IST***A** database management system. |
| FTEE | **F**ull **T**ime **E**quivalent **E**mployee. |
| GUI | **G**raphical **U**ser **I**nterface. The type of interface chosen for BCMA V. 3.0. |
| IV | A medication given intraveneously (within a vein) to a patient from anIV bag. IV types include Admixture, Chemotherapy, Hyperal, Piggyback, and Syringe. |
| Journaling | A record of changes made in files and messages transmitted. It is quite useful when recovering previous versions of a file before updates were made, or to reconstruct updates if an updated file gets damaged. |
| KIDS | **K**ernel **I**nstallation & **D**istribution **S**ystem. |
| MSM | **M**icronectics **S**tandard **M**UMPS. |
| MUMPS | **M**assachusettsGeneral Hospital **U**tility **M**ulti-**P**rogramming **S**ystem. |
| PRN Order | The Latin abbreviation for **P**ro **R**e **N**ata. A medication dosage given to a patient on an “as needed” basis. |
| PSB CPRS MED BUTTON | The name of the security “key” that must be assigned to nurses who document verbal- and phone-type STAT and NOW (One-Time) medication orders using the CPRS Med Order Button on the BCMA VDL. |
| PSB INSTRUCTOR | The name of the security “key” that must be assigned to nursing instructors, supervising nursing students, so they can access user options within BCMA V. 3.0. |

Glossary

|  |  |
| --- | --- |
| Learning BCMAV. 3.0 Lingo (cont.) | The alphabetical listing, in this section, is designed to familiarize you with the many acronyms and terms used throughout this guide. |

Example: Alphabetical Listing of BCMA V. 3.0 Acronyms and Terms

|  |  |
| --- | --- |
| Acronym/Term | Definition |
| PSB MANAGER | The name of the security “key” that must be assigned to managers so they can access the PSB Manager options within BCMA V. 3.0. |
| PSB STUDENT | The name of the security “key” that must be assigned to nursing students, supervised by nursing instructors, so they can access user options within BCMA V. 3.0. This key also requires that a nursing instructor sign on to BCMA. |
| RPC  | **R**emote **P**rocedure **C**all. A procedure stored on the **V***IST***A** Server, which is executed to return data to the Client.  |
| RPC Broker | A Client/Server System within the VA’s Veterans Health Information Systems and Technology Architecture (**V***IST***A**) environment. It enables client applications to communicate and exchange data with M Servers. |
| Security Keys | Used to access specific options within BCMA V. 3.0 that are otherwise “locked” without the security key. Only users designated as “Holders” may access these options. |
| Server | An architecture in which one computer can get information from another. The Server, which can be anything from a personal computer to a mainframe, supplies the requested data or services to the Client. |
| VDL | **V**irtual **D**ue **L**ist. An on-line “list” used by clinicians when administering active medication orders (i.e., Unit Dose, IV Push, IV Piggyback, and large-volume IVs) to a patient. This is the Main Screen in BCMA V. 3.0. **Note:** This is called BCMA VDL in this guide to eliminate confusion with the **V***IST***A** Documentation Library (VDL) also mentioned in this guide. |
| V*IST*A | **V**eterans Health **I**nformation **S**ystems and **T**echnology **A**rchitecture. |
| ZPL | **Z**ebra **P**rogramming **L**anguage. |

# APPENDIX A: Sample KIDS Load & Installation

>**D ^XUP**

Setting up programmer environment

Terminal Type set to: C-VT320

Select OPTION NAME: **XPD MAIN** Kernel Installation & Distribution System

Select Kernel Installation & Distribution System Option: **INSTALL**ation

Select Installation Option: **?**

 1 Load a Distribution

 2 Verify Checksums in Transport Global

 3 Print Transport Global

 4 Compare Transport Global to Current System

 5 Backup a Transport Global

 6 Install Package(s)

 Restart Install of Package(s)

 Unload a Distribution

Select Installation Option: **1** Load a Distribution

Enter a Host File: **PSB\_3\_0.KID**

KIDS Distribution saved on Jan 22, 2004@06:00:58

Comment: BAR CODE MED ADMIN V3

This Distribution contains Transport Globals for the following Package(s):

 PSB 3.0

Distribution OK!

Want to Continue with Load? YES// **<Enter>**

Loading Distribution...

 PSB 3.0

Use INSTALL NAME: **PSB 3.0** to install this Distribution.

APPENDIX A: Sample KIDS Load & Installation

Select Installation Option: **?**

 1 Load a Distribution

 2 Verify Checksums in Transport Global

 3 Print Transport Global

 4 Compare Transport Global to Current System

 5 Backup a Transport Global

 6 Install Package(s)

 Restart Install of Package(s)

 Unload a Distribution

Select Installation Option: **6** Install Package(s)

Select INSTALL NAME: **PSB 3.0** Loaded from Distribution 1/22/04@06:44:48

 => BAR CODE MED ADMIN V3 ;Created on Jan 22, 2004@06:00:58

This Distribution was loaded on Jan 22, 2004@06:44:48 with header of

 BAR CODE MED ADMIN V3 ;Created on Jan 22, 2004@06:00:58

 It consisted of the following Install(s):

 PSB 3.0

Checking Install for Package PSB 3.0

Install Questions for PSB 3.0

Incoming Files:

 53.66 BCMA IV PARAMETERS

Note: You already have the 'BCMA IV PARAMETERS' File.

 53.68 BCMA MISSING DOSE REQUEST

Note: You already have the 'BCMA MISSING DOSE REQUEST' File.

 53.69 BCMA REPORT REQUEST

Note: You already have the 'BCMA REPORT REQUEST' File.

 53.78 BCMA MEDICATION VARIANCE LOG

Note: You already have the 'BCMA MEDICATION VARIANCE LOG' File.

 53.79 BCMA MEDICATION LOG

Note: You already have the 'BCMA MEDICATION LOG' File.

Want KIDS to Rebuild Menu Trees Upon Completion of Install? YES// **NO**

Want KIDS to INHIBIT LOGONs during the install? YES// NO

Want to DISABLE Scheduled Options, Menu Options, and Protocols? YES// **NO**

Enter the Device you want to print the Install messages.

You can queue the install by enter a 'Q' at the device prompt.

Enter a '^' to abort the install.

DEVICE: HOME// **GENERIC INCOMING TELNET**

APPENDIX A: Sample KIDS Load & Installation

 Install Started for PSB 3.0 :

 Jan 22, 2004@06:45:58

Build Distribution Date: Jan 22, 2004

 Installing Routines:

 Jan 22, 2004@06:45:59

 Installing Data Dictionaries:

 Jan 22, 2004@06:46

 Installing PACKAGE COMPONENTS:

 Installing SECURITY KEY

 Installing FORM

 Installing HL LOGICAL LINK

 Installing HL7 APPLICATION PARAMETER

 Installing PROTOCOL

 Installing REMOTE PROCEDURE

 Installing LIST TEMPLATE

 Installing OPTION

 Installing PARAMETER DEFINITION

 Installing PARAMETER TEMPLATE

 Jan 22, 2004@06:46:05

 Updating Routine file...

 Updating KIDS files...

 PSB 3.0 Installed.

 Jan 22, 2004@06:46:06

 Install Message sent #160672

----------------------------------------------------------------------------

 +------------------------------------------------------------+

 100% ¦ 25 50 75 ¦

Complete +------------------------------------------------------------+